{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["設1面"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"設1面","index":0,"n_rows":56,"n_cols":39,"rows_kept":56,"cut":false,"hidden":false,"merged":[[30,17,30,28],[31,17,31,28],[29,34,29,37],[24,9,24,13],[24,4,24,8],[8,9,8,37],[9,9,9,13],[24,22,24,28],[12,4,12,8],[25,34,25,37],[20,4,23,8],[25,22,25,28],[4,8,4,39],[14,34,14,37],[14,15,14,26],[13,34,13,37],[13,15,13,18],[3,8,3,39],[5,8,5,39],[6,8,6,39],[11,31,11,32],[9,14,9,32],[9,33,9,37],[9,4,9,8],[5,0,5,7],[8,4,8,8],[9,38,9,39],[2,9,2,16],[2,21,2,39],[8,38,8,39],[8,0,8,3],[9,0,9,3],[6,0,6,7],[1,0,2,7],[3,0,3,7],[2,17,2,20],[4,0,4,7],[12,25,12,28],[12,20,12,23],[12,15,12,17],[11,26,11,27],[11,21,11,22],[28,34,28,37],[11,16,11,17],[15,15,15,17],[15,19,15,28],[17,22,17,28],[11,4,11,8],[26,34,26,37],[26,22,26,28],[16,4,19,8],[10,31,10,32],[10,26,10,27],[10,21,10,22],[10,16,10,17],[10,4,10,8],[27,4,37,4],[19,22,19,28],[36,17,36,28],[33,17,33,28],[29,17,29,28],[38,17,38,27],[38,34,38,37],[39,34,39,37],[27,17,27,27],[27,34,27,37],[32,34,32,37],[31,34,31,37],[32,17,32,28],[34,17,34,28],[30,34,30,37],[43,34,43,37],[44,34,44,37],[45,34,45,37],[46,34,46,37],[47,34,47,37],[41,0,55,3],[41,4,55,8],[43,18,43,24],[54,34,54,37],[55,34,55,37],[48,34,48,37],[49,34,49,37],[50,34,50,37],[51,34,51,37],[52,34,52,37],[53,34,53,37],[33,34,33,37],[41,18,41,24],[50,18,50,24],[52,18,52,24],[55,18,55,24],[23,22,23,24],[45,18,45,24],[48,18,48,24],[41,34,41,37],[42,34,42,37]],"flags":["formulas_cached_only"]}
["設計内容（現況）説明書"]
["住宅の種類",{"$nulls":7},"□","一戸建ての住宅"]
[{"$nulls":8},"□","共同住宅等の住戸の部分のみ",{"$nulls":7},"（住戸番号"]
["建築物の名称"]
["建築物の所在地"]
["設計者等の氏名"]
["審査員氏名"]
[]
["確認",null,null,null,"確認",{"$nulls":4},"設　計　内　容　（　現　況　）　説　明　欄",{"$nulls":28},"設計内容"]
["事項",null,null,null,"項目",{"$nulls":4},"項　　　　目",{"$nulls":4},"設　計　内　容　（　現　況　）　",{"$nulls":18},"記載図書",{"$nulls":4},"確認欄"]
["基本事項",null,null,null,"外皮性能等",{"$nulls":4},"地域区分",{"$nulls":4},"□",1,"地域",null,null,"□",2,"地域",null,null,"□",3,"地域",null,null,"□",4,"地域",null,"□","計算書"]
[{"$nulls":4},"に係る",{"$nulls":9},"□",5,"地域",null,null,"□",6,"地域",null,null,"□",7,"地域",null,null,"□",8,"地域",null,"□","仕上表"]
[{"$nulls":4},"基本事項",{"$nulls":4},"住宅の構造",{"$nulls":4},"□","木造住宅",null,null,"（","□","軸組構法",null,null,null,"□","枠組構法",null,null,null,"）",null,null,null,"□","建具表"]
[{"$nulls":14},"□","鉄骨造住宅",{"$nulls":17},"□","矩計図"]
[{"$nulls":14},"□","鉄筋コンクリート造（組石造含む。）住宅",{"$nulls":17},"□"]
[null,"　　",{"$nulls":12},"□","その他",null,null,"（",{"$nulls":10},"）"]
["躯体の",null,null,null,"性能基準等",{"$nulls":4},"外皮平均",{"$nulls":4},"外皮平均熱貫流率（UA）",{"$nulls":18},"□","計算書"]
["外皮性能等",{"$nulls":8},"熱貫流率",{"$nulls":9},"（UA",null,"＝",{"$nulls":7},"）",null,null,"【W/㎡K】","□","仕様書"]
[{"$nulls":9},"外皮平均",{"$nulls":4},"冷房期の平均日射熱取得率の計算値（ηAC）",{"$nulls":18},"□","平面図"]
[{"$nulls":9},"日射熱取得率",{"$nulls":9},"（ηAC",null,"＝",{"$nulls":7},"）",null,null,"【―】","□","建具表"]
[{"$nulls":4},"仕様基準",{"$nulls":4},"躯体の断熱",{"$nulls":4},"□","熱貫流率の基準に適合",{"$nulls":17},"□","矩計図"]
[{"$nulls":14},"□","断熱材の熱抵抗値の基準に適合"]
[{"$nulls":14},"□","構造熱橋部の基準に適合（鉄筋コンクリート造等の場合）"]
[{"$nulls":9},"開口部の断熱",{"$nulls":4},"□","開口部比率の区分：",{"$nulls":5},"（",null,null,null,"）"]
["一次",null,null,null,"基本事項",{"$nulls":4},"居室の面積",{"$nulls":4},"延床面積",{"$nulls":6},"（",{"$nulls":7},"）","㎡",null,null,"□","計算書"]
["エネルギー",{"$nulls":14},"主たる居室",{"$nulls":5},"（",{"$nulls":7},"）","㎡",null,null,"□","仕上げ表"]
["消費量",null,null,"　",{"$nulls":11},"その他の居室",{"$nulls":5},"（",{"$nulls":7},"）","㎡",null,null,"□","建具表"]
[{"$nulls":4},"性能基準","外皮",null,null,null,"断熱性能等",{"$nulls":4},"□",null,"（","一次エネルギー消費量計算結果による",{"$nulls":12},"）",null,null,"□","認定書"]
[{"$nulls":33},"□"]
[{"$nulls":5},"暖冷房設備",null,null,null,"暖房方式",{"$nulls":4},"□",null,"（","一次エネルギー消費量計算結果による",{"$nulls":11},"）",null,null,null,"□","仕上げ表"]
[{"$nulls":9},"冷房方式",{"$nulls":4},"□",null,"（","一次エネルギー消費量計算結果による",{"$nulls":11},"）",null,null,null,"□","仕様書"]
[{"$nulls":5},"換気設備",null,null,null,"換気設備方式",{"$nulls":4},"□",null,"（","一次エネルギー消費量計算結果による",{"$nulls":11},"）",null,null,null,"□","平面図"]
[{"$nulls":5},"給湯設備",null,null,null,"給湯設備",{"$nulls":4},"□",null,"（","一次エネルギー消費量計算結果による",{"$nulls":11},"）",null,null,null,"□","設備図"]
[{"$nulls":5},"照明設備",null,null,null,"照明器具",{"$nulls":4},"□",null,"（","一次エネルギー消費量計算結果による",{"$nulls":11},"）",null,null,null,"□","カタログ等"]
[{"$nulls":5},"太陽光発電",null,null,null,"太陽光発電の",{"$nulls":4},"□",null,"（","一次エネルギー消費量計算結果による",{"$nulls":11},"）"]
[{"$nulls":9},"使用について"]
[{"$nulls":5},"ｺｰｼﾞｪﾈﾚｰｼｮﾝ",null,null,null,"ｺｰｼﾞｪﾈﾚｰｼｮﾝの",{"$nulls":4},"□",null,"（","一次エネルギー消費量計算結果による",{"$nulls":11},"）"]
[{"$nulls":9},"使用について"]
[{"$nulls":4},"設備ごとの仕様基準",{"$nulls":9},"□",null,"（","設備ごとの仕様基準による",{"$nulls":11},"）",null,null,null,"□","仕上げ表"]
[{"$nulls":33},"□","仕様書"]
[{"$nulls":33},"□"]
["住宅の「ＺＥＨマーク」「ゼロエネ相当」に関する事項",null,null,null,"住宅の「住宅の｢ZEHマーク｣、｢ゼロエネ相当｣に関する表示\n\n※選択した場合のみ\n",{"$nulls":4},"外皮基準",{"$nulls":4},"基準値",null,null,"（",{"$nulls":7},"）",null,null,null,"【W/m2K】",null,null,null,"□","計算書"]
[{"$nulls":9},"再生可能エネル",{"$nulls":4},"・再生可能ｴﾈﾙｷﾞｰを除いた設計一次ｴﾈﾙｷﾞｰ消費量（その他除く）",{"$nulls":18},"□"]
[{"$nulls":9},"ギー除き",{"$nulls":7},"（",{"$nulls":7},"）","GJ/年　･･･②",{"$nulls":6},"□"]
[{"$nulls":14},"・再生可能ｴﾈﾙｷﾞｰを除いた一次ｴﾈﾙｷﾞｰ消費削減量（その他除く）",{"$nulls":18},"□"]
[{"$nulls":17},"（",{"$nulls":7},"）","GJ/年　･･･③=①-②",{"$nulls":6},"□"]
[{"$nulls":14},"・再生可能ｴﾈﾙｷﾞｰを除いた設計一次ｴﾈﾙｷﾞｰ消費量（その他除く）"]
[{"$nulls":14},"の基準一次ｴﾈﾙｷﾞｰ消費量（その他除く）からの削減率"]
[{"$nulls":17},"（",{"$nulls":7},"）","％削減　･･･③/①×100"]
[{"$nulls":9},"再生可能エネル",{"$nulls":4},"・再生可能ｴﾈﾙｷﾞｰを加えた設計一次ｴﾈﾙｷﾞｰ消費量（その他除く）"]
[{"$nulls":9},"ギー加え",{"$nulls":7},"（",{"$nulls":7},"）","GJ/年　･･･④"]
[{"$nulls":14},"・再生可能ｴﾈﾙｷﾞｰを加えた一次ｴﾈﾙｷﾞｰ消費削減量（その他除く）"]
[{"$nulls":17},"（",{"$nulls":7},"）","GJ/年　･･･⑤=①-④"]
[{"$nulls":14},"・再生可能ｴﾈﾙｷﾞｰを加えた設計一次ｴﾈﾙｷﾞｰ消費量（その他除く）"]
[{"$nulls":14},"の基準一次ｴﾈﾙｷﾞｰ消費量（その他除く）からの削減率"]
[{"$nulls":17},"（",{"$nulls":7},"）","％削減　･･･⑤/①×100"]