{"text_format":"2","workbook":"xls","n_sheets":7,"sheets":["断熱等性能","一次エネルギー消費量","耐久性・可変性","耐震","高齢者等級3","高齢者等級4","高齢者等級5"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":14,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"断熱等性能","index":0,"n_rows":30,"n_cols":37,"rows_kept":30,"cut":false,"hidden":false,"merged":[[1,0,1,13],[1,14,1,36],[2,0,2,13],[2,14,2,36],[4,0,4,6],[4,8,4,34],[6,35,7,36],[7,1,7,4],[7,7,7,9],[7,10,7,13],[7,14,7,30],[7,31,7,34],[10,11,10,13],[11,12,13,13],[6,1,6,4],[6,5,7,6],[6,7,6,9],[6,10,6,34],[26,10,26,13],[17,12,17,13],[17,19,17,26],[11,3,11,4],[12,16,12,20],[8,0,23,0],[9,1,9,4],[10,1,10,4],[8,7,8,9],[9,7,9,9],[8,10,8,13],[17,32,17,34],[18,12,19,13],[18,32,18,34],[20,12,23,13],[9,10,9,13],[11,7,16,11],[17,7,23,11],[14,12,16,13],[15,16,15,20],[28,10,28,13],[29,20,29,29],[24,7,24,9],[24,10,24,13],[26,20,26,29],[26,32,26,34],[27,10,27,13],[27,32,27,34],[25,7,25,9],[25,10,25,13]],"flags":["formulas_cached_only"]}
["設計内容説明書【断熱等性能等級】",{"$nulls":35},"現金取得者向け新築対象住宅証明書用"]
["評価対象建築物の名称"]
["評価対象建築物の所在地"]
[]
["対象とする証明基準",{"$nulls":6},"■","評価方法基準第5　5　5-1（3）【断熱等性能等級】　等級４"]
[]
[null,"性能表示　　　　",null,null,null,"自己\n評価\n結果",null,"確認",null,null,"設計内容説明欄",{"$nulls":24},"設計\n内容\n確認欄"]
[null,"事項",{"$nulls":5},"項目",null,null,"項目",null,null,null,"設計内容",{"$nulls":16},"記載図書"]
["５温熱環境・エネルギー消費量","５－１",null,null,null,"等級",null,"適用する",null,null,"適用する基準",null,null,null,"□","性能基準"]
[null,"断熱等",null,null,null,"■",4,"基準",{"$nulls":6},"□","仕様基準"]
[null,"性能等級"]
[null,"（",null,"）地域",null,null,null,"性能基準を適用する場合",{"$nulls":4},"外皮平均熱貫流率",null,"□","外皮平均熱貫流率　UA",{"$nulls":15},"□","仕上表"]
[{"$nulls":15},"(",{"$nulls":5},"W/㎡K",null,"）",{"$nulls":7},"□","平面図"]
[{"$nulls":31},"□","立面図"]
[{"$nulls":12},"冷房期の平均日射熱取得率",null,"□","冷房期の平均日射熱取得率　ηA",{"$nulls":15},"□","矩計図"]
[{"$nulls":15},"(",{"$nulls":6},"）",{"$nulls":8},"□","建具表"]
[{"$nulls":31},"□","計算書"]
[{"$nulls":7},"仕様基準を適用する場合",{"$nulls":4},"適用条件",null,"開口部比率",null,null,null,"（",{"$nulls":8},"）",null,null,null,"□"]
[{"$nulls":12},"躯体の断熱",null,"□","熱貫流率の基準に適合",{"$nulls":15},"□"]
[{"$nulls":14},"□","熱抵抗値の基準に適合"]
[{"$nulls":12},"開口部の断熱及び日射",null,"開口部比率の区分"]
[{"$nulls":14},"□","区分（い）",null,null,"□","区分（ろ）",null,null,"□","区分（は）",null,null,"□","区分（に）"]
[{"$nulls":14},"□","緩和措置有り"]
[{"$nulls":15},"□","窓の断熱（2％緩和）",{"$nulls":5},"□","窓の日射（4％緩和）"]
[{"$nulls":7},"結露防止",null,null,"繊維系断熱材",null,null,null,"・","繊維系断熱材等の使用",{"$nulls":5},"（","□","有",null,"□","無　）",{"$nulls":4},"□","仕上表"]
[{"$nulls":7},"対策",null,null,"防湿層",null,null,null,"・","防湿層の設置",{"$nulls":5},"（","□","有",null,"□","無　）",{"$nulls":4},"□","矩計図"]
[{"$nulls":10},"の設置",null,null,null,"□","除外規定適用",null,null,null,"（",{"$nulls":10},"）","□"]
[{"$nulls":10},"通気層",null,null,null,"・","通気層の設置",{"$nulls":5},"（","□","有",null,"□","無　）",{"$nulls":4},"□"]
[{"$nulls":10},"の設置",null,null,null,"・","防風層の設置",{"$nulls":5},"（","□","有",null,"□","無　）"]
[{"$nulls":14},"□","除外規定適用",null,null,null,"（",{"$nulls":10},"）"]

{"sheet":"一次エネルギー消費量","index":1,"n_rows":67,"n_cols":37,"rows_kept":67,"cut":false,"hidden":false,"merged":[[7,30,7,33],[56,6,58,6],[15,13,15,15],[20,18,20,26],[32,17,32,28],[50,6,55,6],[6,0,6,3],[6,4,7,5],[6,6,6,8],[6,9,6,33],[7,0,7,3],[15,6,23,6],[1,0,1,13],[1,14,1,36],[2,0,2,13],[2,14,2,36],[4,0,4,6],[6,34,7,35],[7,6,7,8],[7,9,7,12],[7,13,7,29],[8,6,9,12],[11,6,11,8],[10,20,10,25],[11,20,11,25],[12,20,12,25],[13,9,14,12],[13,6,14,8],[15,7,18,12],[19,7,23,12],[52,19,52,28],[60,22,60,28],[66,15,66,27],[59,6,66,6],[39,6,49,6],[34,6,38,6],[24,6,28,6],[27,17,27,28]],"flags":["formulas_cached_only"]}
["設計内容説明書【一次エネルギー消費量】",{"$nulls":35},"現金取得者向け新築対象住宅証明書用"]
["評価対象建築物の名称"]
["評価対象建築物の所在地"]
[]
["対象とする証明基準",{"$nulls":6},"■","評価方法基準第5　5　5-2（3）【一次エネルギー消費量等級】　等級４以上"]
[]
["性能表示　　　　",null,null,null,"自己\n評価\n結果",null,"確認",null,null,"設計内容説明欄",{"$nulls":24},"設計\n内容\n確認欄"]
["事項",{"$nulls":5},"項目",null,null,"項目",null,null,null,"設計内容",{"$nulls":16},"記載図書"]
["５－２",null,null,null,"等級",null,"適用する基準",{"$nulls":6},"□","性能基準",{"$nulls":15},"□","仕上表"]
["一次エネルギー",null,null,null,"□",5,{"$nulls":7},"□","仕様基準（等級４のみ）",{"$nulls":15},"□","平面図"]
["消費量等級",null,null,null,"□",4,{"$nulls":7},"延べ床面積",{"$nulls":5},"（",{"$nulls":6},"）","㎡",null,null,"□","立面図"]
[{"$nulls":6},"基本事項",null,null,"居室の面積",{"$nulls":4},"主たる居室",{"$nulls":4},"（",{"$nulls":6},"）","㎡",null,null,"□","矩計図"]
["地域区分",{"$nulls":13},"その他の居室",{"$nulls":4},"（",{"$nulls":6},"）","㎡",null,null,"□","建具表"]
["（",null,"）",null,null,null,"外皮",null,null,"適用する基準",null,null,null,"□","性能基準",{"$nulls":15},"□","計算書"]
[{"$nulls":13},"□","仕様基準（等級４のみ）",{"$nulls":15},"□"]
[{"$nulls":6},"外皮","自然風の利用",{"$nulls":5},"主たる居室",null,null,"□","なし"]
[{"$nulls":16},"□","あり(5回/h相当以上）",{"$nulls":5},"□","あり(20回/h相当以上）"]
[{"$nulls":13},"その他の",null,null,"□","なし"]
[{"$nulls":13},"居室",null,null,"□","あり(5回/h相当以上）",{"$nulls":5},"□","あり(20回/h相当以上）"]
[{"$nulls":7},"蓄熱の利用",{"$nulls":5},"□","利用なし"]
[{"$nulls":13},"□","利用あり",null,null,"（",{"$nulls":9},"）"]
[{"$nulls":14},"利用ありの場合　暖房期日射地域区分"]
[{"$nulls":15},"□","H１区分",null,null,null,"□","H２区分",null,null,"□","H３区分"]
[{"$nulls":15},"□","H４区分",null,null,null,"□","H５区分"]
[{"$nulls":6},"暖冷房設備","暖房",null,"暖房方式の",null,null,null,"□","ダクト式セントラル空調を用いて、住宅全体を暖房する",{"$nulls":15},"□","機器表"]
[{"$nulls":7},"設備",null,"選択",null,null,null,"□","「主たる居室」と「その他の居室」の両方あるいはいずれかに",{"$nulls":15},"□","仕様書"]
[{"$nulls":14},"暖房設備機器または放熱器を設置する",{"$nulls":15},"□","平面図"]
[{"$nulls":14},"種類",null,"（",{"$nulls":12},")","□"]
[{"$nulls":13},"□","暖房設備機器または放熱器を設置しない",{"$nulls":15},"□"]
[{"$nulls":7},"冷房",null,"冷房方式の",null,null,null,"□","ダクト式セントラル空調を用いて、住宅全体を冷房する"]
[{"$nulls":7},"設備",null,"選択",null,null,null,"□","「主たる居室」と「その他の居室」の両方あるいはいずれかに"]
[{"$nulls":14},"冷房設備機器を設置する"]
[{"$nulls":14},"種類",null,"（",{"$nulls":12},")"]
[{"$nulls":13},"□","冷房設備機器を設置しない"]
[{"$nulls":6},"換気設備","換気",null,"換気設備の",null,null,null,"□","ダクト式第１種換気設備",{"$nulls":15},"□","機器表"]
[{"$nulls":9},"方式",null,null,null,"□","ダクト式第２種または第3種換気設備",{"$nulls":15},"□","仕様書"]
[{"$nulls":13},"□","壁付け式第１種換気設備",{"$nulls":15},"□","平面図"]
[{"$nulls":13},"□","壁付け式第２種または第３種換気設備",{"$nulls":15},"□"]
[{"$nulls":7},"熱交換",{"$nulls":5},"熱交換型換気設備の有無",{"$nulls":7},"□","あり",null,"□","なし"]
[{"$nulls":6},"給湯設備","給湯",null,"給湯熱源機",null,null,null,"□","ガス給湯機",{"$nulls":8},"□","石油給湯機",{"$nulls":5},"□","機器表"]
[{"$nulls":13},"□","ヒートポンプ・ガス瞬間式併用型給湯機",{"$nulls":15},"□","仕様書"]
[{"$nulls":13},"□","電気ヒーター温水器",{"$nulls":8},"□","電気ヒートポンプ給湯機",{"$nulls":5},"□","平面図"]
[{"$nulls":13},"□","コージェネレーションを使用する",{"$nulls":8},"□","その他の給湯設備機器",{"$nulls":5},"□"]
[{"$nulls":13},"□","給湯設備機器を設置しない"]
[{"$nulls":9},"ふろ機能の",null,null,null,"□","給湯単機能"]
[{"$nulls":9},"種類 ",null,null,null,"□","ふろ給湯機（追焚なし）",{"$nulls":8},"□","ふろ給湯機（追焚あり）"]
[{"$nulls":9},"配管について",null,null,null,"□","先分岐方式",{"$nulls":8},"□","ヘッダー方式"]
[{"$nulls":9},"水栓について",null,null,null,"台所水栓",{"$nulls":4},"□"," 2バルブ水栓",null,null,null,"□","2バルブ水栓以外"]
[{"$nulls":13},"浴室シャワー水栓",{"$nulls":4},"□"," 2バルブ水栓",null,null,null,"□","2バルブ水栓以外"]
[{"$nulls":13},"洗面水栓",{"$nulls":4},"□"," 2バルブ水栓",null,null,null,"□","2バルブ水栓以外"]
["５－２",null,null,null,"等級",null,"給湯設備","給湯",null,"浴槽について",null,null,null,"□","高断熱浴槽を使用しない",{"$nulls":6},"□","高断熱浴槽を使用する",{"$nulls":7},"□","機器表"]
["一次エネルギー",null,null,null,"□",5,null,null,null,"太陽熱給湯",null,null,null,"□","採用なし",{"$nulls":15},"□","仕様書"]
["消費量等級",null,null,null,"□",4,null,null,null,"の採用に",null,null,null,"□","採用あり",null,null,null,"（",{"$nulls":10},"）","□","平面図"]
[{"$nulls":9},"ついて",null,null,null,"採用する場合　年間日射地域区分",{"$nulls":16},"□"]
[{"$nulls":14},"□","A１区分",null,null,null,"□","A２区分",null,null,null,"□","A３区分",{"$nulls":4},"□"]
[{"$nulls":14},"□","A４区分",null,null,null,"□","A５区分"]
[{"$nulls":4},"　　",null,"照明","照明",null,"照明器具",null,null,null,"主たる居室",null,null,null,"□","設置あり",{"$nulls":4},"□","設置なし",{"$nulls":5},"□","機器表"]
[{"$nulls":13},"その他の居室",null,null,null,"□","設置あり",{"$nulls":4},"□","設置なし",{"$nulls":5},"□","仕様書"]
[{"$nulls":13},"非居室",null,null,null,"□","設置あり",{"$nulls":4},"□","設置なし",{"$nulls":5},"□","平面図"]
[{"$nulls":6},"発電","太陽",null,"太陽光発電",null,null,null,"□","太陽光発電を採用しない",{"$nulls":15},"□","機器表"]
[{"$nulls":7},"光発",null,"設備の採用",null,null,null,"□","太陽光発電を採用する",{"$nulls":6},"（",{"$nulls":7},"）","□","仕様書"]
[{"$nulls":7},"電",null,"について",null,null,null,"採用する場合　年間日射地域区分",{"$nulls":16},"□","立面図"]
[{"$nulls":14},"□","A１区分",null,null,null,"□","A２区分",null,null,null,"□","A３区分",{"$nulls":4},"□"]
[{"$nulls":14},"□","A４区分",null,null,null,"□","A５区分"]
[{"$nulls":7},"コジェネ",null,"コージェネ",null,null,null,"□","コージェネレーションを採用しない",{"$nulls":15},"□","機器表"]
[{"$nulls":9},"レーション",null,null,null,"□","コージェネレーションを採用する",{"$nulls":15},"□","仕様書"]
[{"$nulls":9},"の種類について",{"$nulls":4},"（",{"$nulls":13},"）"]

{"sheet":"耐久性・可変性","index":2,"n_rows":46,"n_cols":37,"rows_kept":46,"cut":false,"hidden":false,"merged":[[1,0,1,13],[1,14,1,36],[2,0,2,13],[2,14,2,36],[4,0,5,6],[35,20,35,29],[34,7,34,9],[34,10,34,13],[5,8,5,34],[4,8,4,34],[45,32,45,34],[42,7,42,9],[42,10,42,13],[37,32,37,34],[39,32,39,34],[45,7,45,9],[45,10,45,13],[43,32,43,34],[44,7,44,9],[40,10,40,13],[41,10,41,13],[41,32,41,34],[44,10,44,13],[39,7,39,9],[39,10,39,13],[40,7,40,9],[43,7,43,9],[43,10,43,13],[36,0,45,0],[36,7,36,9],[36,10,36,13],[37,1,37,4],[37,10,37,13],[38,1,38,4],[38,7,38,9],[38,10,38,13],[39,1,39,4],[41,7,41,9],[30,10,30,13],[30,24,30,29],[31,32,31,34],[33,7,33,9],[33,10,33,13],[35,10,35,13],[34,32,34,34],[35,7,35,9],[30,7,30,9],[26,32,26,34],[27,18,27,29],[28,7,28,9],[28,10,28,13],[28,32,28,34],[29,7,29,9],[29,10,29,13],[22,7,22,9],[22,18,22,29],[22,32,22,34],[24,19,24,23],[24,25,24,29],[25,7,25,9],[25,10,25,13],[12,32,12,34],[15,19,15,29],[16,7,16,9],[16,10,16,13],[17,10,17,13],[19,19,19,29],[19,32,19,34],[9,0,32,0],[9,7,9,9],[9,10,9,13],[10,1,10,4],[10,7,10,9],[10,10,10,13],[11,1,11,4],[12,1,12,4],[20,7,20,9],[20,10,20,13],[7,1,7,4],[7,5,8,6],[7,7,7,9],[7,10,7,34],[7,35,8,36],[8,1,8,4],[8,7,8,9],[8,10,8,13],[8,14,8,30],[8,31,8,34]],"flags":["formulas_cached_only"]}
["設計内容説明書【耐久性・可変性】",{"$nulls":35},"現金取得者向け新築対象住宅証明書用"]
["評価対象建築物の名称"]
["評価対象建築物の所在地"]
[]
["対象とする証明基準",{"$nulls":6},"■","評価方法基準第5　3　3-1（3）【劣化対策等級】　等級３　"]
[{"$nulls":7},"■","評価方法基準第5　4　4-1（3）【維持管理対策等級（専用配管）】　等級2以上　"]
[]
[null,"性能表示　　　　",null,null,null,"自己\n評価\n結果",null,"確認",null,null,"設計内容説明欄",{"$nulls":24},"設計\n内容\n確認欄"]
[null,"事項",{"$nulls":5},"項目",null,null,"項目",null,null,null,"設計内容",{"$nulls":16},"記載図書"]
["３劣化の軽減","３－１",null,null,null,"等級",null,"外壁の",null,null,"外壁の構造等",null,null,null,"□","外壁通気構造等",{"$nulls":15},"□","仕上表"]
[null,"劣化対策",null,null,null,"■",3,"軸組等",null,null,"（地面から１m）",{"$nulls":4},"□","製材、集成材等又は構造用合板等＋薬剤処理（現場処理）",{"$nulls":14},"□","矩計図"]
[null,"等級",{"$nulls":13},"□","製材、集成材等＋小径13.5㎝",{"$nulls":14},"□","伏図等"]
[null,"（構造躯体等）",{"$nulls":13},"□","製材、集成材等＋耐久性区分Ｄ1＋小径12.0㎝以上",{"$nulls":14},"□"]
[{"$nulls":15},"□","耐久性区分Ｄ１のうち、ヒノキ等の高耐久樹種"]
[null,"　　",{"$nulls":12},"□","Ｋ３以上の薬剤処理（工場処理）"]
[{"$nulls":14},"□","その他",null,null,"（","　",{"$nulls":10},"）"]
[{"$nulls":7},"土台",null,null,"防腐・防蟻",null,null,null,"□","土台に接する外壁下端水切り",{"$nulls":15},"□","仕上表"]
[{"$nulls":10},"処理",null,null,null,"□","Ｋ３以上の薬剤処理（工場処理）",{"$nulls":15},"□","矩計図"]
[{"$nulls":14},"□","耐久性区分Ｄ１のうち、ヒノキ等の高耐久樹種",{"$nulls":15},"□","伏図等"]
[{"$nulls":14},"□","その他",null,null,"（","　",{"$nulls":10},"）","□"]
[{"$nulls":7},"浴室・脱衣",null,null,"防水上の措置",null,null,null,"□","浴室",null,"□","防水上有効な仕上げ",{"$nulls":5},"□","浴室ユニット",{"$nulls":5},"□","仕上表"]
[{"$nulls":7},"室の防水",{"$nulls":9},"□","外壁軸組等の防腐措置等",{"$nulls":12},"□","平面図"]
[{"$nulls":15},"方法：",null,"（",{"$nulls":12},"）","□"]
[{"$nulls":14},"□","脱衣室",null,"□","防水上有効な仕上げ",{"$nulls":4},"□","外壁軸組等の防腐措置等"]
[{"$nulls":15},"方法：",null,"（","床",{"$nulls":5},"壁",{"$nulls":5},"）"]
[{"$nulls":7},"地盤",null,null,"防蟻措置",null,null,null,"・","防蟻措置",{"$nulls":6},"（","□","有",null,"□","対象区域外）",null,null,null,"□","矩計図"]
[{"$nulls":15},"□","べた基礎等",null,null,null,"□","土壌処理",null,null,null,"□","その他",{"$nulls":4},"□"]
[{"$nulls":15},"方法：",null,"（","　",{"$nulls":11},"）"]
[{"$nulls":7},"基礎高さ",null,null,"基礎高さ",null,null,null,"□","地面から基礎上端又は土台下端までの高さが400mm以上"]
[{"$nulls":7},"床下防湿",null,null,"床下地盤面の",null,null,null,"□","防湿方法",null,null,"〔","□","コンクリート",null,null,null,"□","防湿フィルム",{"$nulls":5},"□","矩計図"]
[{"$nulls":7},"措置等",null,null,"防湿措置",{"$nulls":8},"□","その他",null,null,"（",{"$nulls":6},"）〕","□","伏図等"]
[{"$nulls":10},"床下換気措置",null,null,null,"□","換気措置",null,null,"〔","□","換気口",null,null,"□","ねこ土台",null,null,"□","その他",null,"〕","□"]
[{"$nulls":14},"□","基礎断熱工法"]
[{"$nulls":7},"小屋裏",null,null,"小屋裏換気",null,null,null,"・","小屋裏の有無",{"$nulls":8},"（","□","有",null,"□","無","）","□","立面図"]
[{"$nulls":7},"換気",null,null,"の措置",null,null,null,"・","小屋裏換気設置の有無",{"$nulls":8},"（","□","有",null,"□","無","）","□"]
[{"$nulls":7},"認定書等",null,null,"認定書等活用",null,null,null,"□","認定書等の活用",null,null,null,"（",{"$nulls":10},"）"]
["４維持管理・更新への配慮","４－１",null,null,null,"等級",null,"専用配管",null,null,"コンクリート",null,null,null,"□","すべての評価対象配管がコンクリート内に埋込まれていない",{"$nulls":15},"□","平面図"]
[null,"維持管理",null,null,null,"□",3,null,null,null,"内埋込み配管",{"$nulls":20},"□"]
[null,"対策等級",null,null,null,"■",2,"地中",null,null,"埋設管上の",null,null,null,"・","地中埋設管上のコンクリート打設",{"$nulls":15},"□","配置図"]
[null,"（専用配管）",{"$nulls":5},"埋設管",null,null,"ｺﾝｸﾘｰﾄ打設",null,null,null,"（","□","無",null,"□","土間コンその他のみ有",{"$nulls":6},"□","対象区域外）",null,null,null,"□"]
[{"$nulls":7},"排水管の",null,null,"内面の仕様",null,null,null,"□","排水管内面が平滑である",{"$nulls":15},"□","仕上表"]
[{"$nulls":7},"性状等",null,null,"設置状態",null,null,null,"□","たわみ、抜け等が生じないよう設置",{"$nulls":15},"□"]
[{"$nulls":7},"専用",null,null,"排水管の",null,null,null,"□","便所、その他水廻りに必要な清掃措置の確保",{"$nulls":15},"□","平面図"]
[{"$nulls":7},"排水管",null,null,"清掃措置",{"$nulls":15},"※等級3のみ",{"$nulls":4},"□"]
[{"$nulls":7},"配管",null,null,"主要接合部等",null,null,null,"□","主要接合部等の点検措置等の確保",{"$nulls":15},"□","平面図"]
[{"$nulls":7},"点検口",null,null,"の点検措置",{"$nulls":15},"※等級3のみ",{"$nulls":4},"□"]

{"sheet":"耐震","index":3,"n_rows":22,"n_cols":37,"rows_kept":22,"cut":false,"hidden":false,"merged":[[21,20,21,29],[12,1,12,4],[4,0,5,6],[4,8,4,34],[5,8,5,34],[19,1,19,4],[20,1,20,4],[21,1,21,4],[18,10,18,13],[18,20,18,29],[22,1,22,4],[12,32,12,34],[17,19,17,29],[16,19,16,29],[19,10,19,13],[11,32,11,34],[13,19,13,29],[15,10,15,13],[11,19,11,29],[14,19,14,29],[1,14,1,36],[1,0,1,13],[2,0,2,13],[8,1,8,4],[7,5,8,6],[8,10,8,13],[7,1,7,4],[2,14,2,36],[13,1,13,4],[7,35,8,36],[7,10,7,34],[8,14,8,30],[8,31,8,34],[8,7,8,9],[9,1,9,4],[12,10,12,13],[7,7,7,9],[9,0,21,0],[9,10,9,13],[9,7,9,9],[21,10,21,13],[17,1,17,4],[10,7,10,9],[11,7,11,9],[10,10,10,13],[11,1,11,4],[10,1,10,4]],"flags":["formulas_cached_only"]}
["設計内容説明書【耐震】",{"$nulls":35},"現金取得者向け新築対象住宅証明書用"]
["評価対象建築物の名称"]
["評価対象建築物の所在地"]
[]
["対象とする証明基準",{"$nulls":6},"■","評価方法基準第5　１　1-1（3）【耐震等級（構造躯体の倒壊等防止）】　等級２若しくは等級３　"]
[{"$nulls":7},"□","評価方法基準第5　１　1-3（3）【その他（地震に対する構造躯体の倒壊等防止及び損傷防止）】　"]
[]
[null,"性能表示　　　　",null,null,null,"自己\n評価\n結果",null,"確認",null,null,"設計内容説明欄",{"$nulls":24},"設計\n内容\n確認欄"]
[null,"事項",{"$nulls":5},"項目",null,null,"項目",null,null,null,"設計内容",{"$nulls":16},"記載図書"]
["1構造の安定","１－１",null,null,null,"等級",null,"構造躯体",null,null,"地震力及び",null,null,null,"□","壁量計算による（階数が２以下の木造の建築物における基準）",{"$nulls":15},"□","伏図"]
[null,"耐震等級",null,null,null,"□",3,"及び",null,null,"風圧力",null,null,null,"□","許容応力度計算による(ルート1)",{"$nulls":15},"□","計算書"]
[{"$nulls":5},"□",2,"基礎等",{"$nulls":6},"□","その他",null,null,"（",{"$nulls":11},"）","□"]
[{"$nulls":10},"基礎",null,null,null,"□","許容応力度計算による"]
[{"$nulls":14},"□","スパン表",null,null,"（",{"$nulls":11},"）"]
[{"$nulls":14},"□","その他",null,null,"（",{"$nulls":11},"）"]
[{"$nulls":10},"横架材",null,null,null,"□","許容応力度計算による"]
[{"$nulls":14},"□","スパン表",null,null,"（",{"$nulls":11},"）"]
[{"$nulls":14},"□","その他",null,null,"（",{"$nulls":11},"）"]
[{"$nulls":10},"認定書等活用",null,null,null,"□","認定書等の活用",null,null,null,"（",{"$nulls":10},"）"]
[null,"１－３",{"$nulls":8},"免震建築物",null,null,null,"□","平成12年建設省告示第2009号第1第3号による免震建築物"]
[null,"その他",{"$nulls":12},"□","免震層及び免震材料の維持管理に関する図書の作成"]
[{"$nulls":10},"認定書等活用",null,null,null,"□","認定書等の活用",null,null,null,"（",{"$nulls":10},"）"]

{"sheet":"高齢者等級3","index":4,"n_rows":41,"n_cols":37,"rows_kept":41,"cut":false,"hidden":false,"merged":[[6,1,6,4],[6,5,7,6],[6,7,6,9],[6,10,6,34],[6,35,7,36],[7,1,7,4],[7,7,7,9],[7,10,7,13],[7,14,7,30],[7,31,7,34],[1,0,1,13],[1,14,1,36],[2,0,2,13],[2,14,2,36],[4,0,4,6],[4,8,4,34],[8,0,18,0],[8,7,8,9],[8,10,8,13],[8,19,8,20],[8,24,8,29],[9,1,9,4],[9,7,9,9],[9,10,9,13],[13,10,13,13],[17,11,17,13],[9,32,9,34],[10,1,10,4],[10,15,10,16],[11,7,11,9],[11,10,11,13],[12,10,12,13],[12,32,12,34],[13,32,13,34],[14,16,14,19],[14,21,14,25],[14,27,14,30],[15,10,15,13],[16,7,16,9],[16,10,16,13],[17,14,17,30],[17,32,17,34],[18,10,18,13],[18,32,18,34],[19,11,19,13],[20,10,20,13],[21,7,21,9],[21,10,21,13],[28,22,28,24],[25,11,25,13],[22,32,22,34],[23,10,23,13],[23,26,23,30],[23,32,23,34],[24,10,24,13],[24,26,24,30],[24,32,24,34],[35,32,35,34],[29,7,29,9],[29,10,29,13],[30,7,30,9],[30,10,30,13],[30,32,30,34],[32,7,32,9],[32,10,32,13],[29,15,29,30],[40,7,40,9],[40,10,40,13],[33,7,33,9],[34,7,34,9],[34,10,34,13],[35,7,35,9],[35,10,35,13],[37,15,37,21],[37,7,37,9],[38,7,38,9],[26,26,26,30],[27,14,27,16],[27,19,27,21],[27,23,27,25]],"flags":["formulas_cached_only"]}
["設計内容説明書【高齢者】",{"$nulls":35},"現金取得者向け新築対象住宅証明書用"]
["評価対象建築物の名称"]
["評価対象建築物の所在地"]
[]
["対象とする証明基準",{"$nulls":6},"■","　評価方法基準第5　9　9-1（3）【高齢者等配慮対策等級】　等級３　"]
[]
[null,"性能表示　　　　",null,null,null,"自己\n評価\n結果",null,"確認",null,null,"設計内容説明欄",{"$nulls":24},"設計\n内容\n確認欄"]
[null,"事項",{"$nulls":5},"項目",null,null,"項目",null,null,null,"設計内容",{"$nulls":16},"記載図書"]
["９高齢者等への配慮","９－１",null,null,null,"等級",null,"部屋の",null,null,"特定寝室",null,null,null,"・","特定寝室",null,null,"（",null,null,"階、室名：",{"$nulls":8},"）","□","平面図"]
[null,"高齢者等配",null,null,null,"■",3,"配置等",null,null,"の位置",null,null,null,"・","特定寝室の存する階にある部屋",{"$nulls":15},"□"]
[null,"慮対策等級",{"$nulls":12},"□","便所"]
[null,"（専用部分）",{"$nulls":5},"段差",null,null,"日常生活",null,null,null,"□","日常生活空間内の床が段差のない構造",{"$nulls":15},"□","平面図"]
[{"$nulls":10},"空間内",null,null,null,"・","適用除外の段差",{"$nulls":15},"□"]
[{"$nulls":15},"□","玄関出入口",null,null,null,"□","玄関上りかまち",{"$nulls":4},"□","浴室出入口"]
[{"$nulls":15},"□","勝手口出入口",null,null,null,"□","バルコニー出入口",{"$nulls":4},"□","ﾀﾀﾐｺｰﾅｰ"]
[{"$nulls":10},"日常生活空間外",null,null,null,"□","日常生活空間外の床が段差のない構造"]
[{"$nulls":7},"階段",null,null,"勾配等",null,null,null,"□","階段の勾配等の基準に適合",{"$nulls":15},"□","平面図"]
[{"$nulls":7},"□","階段無",null,"□","ﾎｰﾑｴﾚﾍﾞｰﾀｰ",null,null,"勾配22/21以下、550㎜≦けあげ×2＋踏面≦650㎜、かつ、踏面195㎜以上",{"$nulls":16},"□"]
[{"$nulls":10},"蹴込み",null,null,null,"□","蹴込みが30mm以下",{"$nulls":15},"□"]
[{"$nulls":10},"□","ﾎｰﾑｴﾚﾍﾞｰﾀｰ"]
[{"$nulls":10},"階段の幅員等",null,null,null,"□","建築基準法施行令第23条から第27条までに定める基準に適合"]
[{"$nulls":7},"手摺",null,null,"手摺の設置",{"$nulls":4},"□","階段",null,null,"□","便所",null,null,"□","浴室（浴槽出入り）",{"$nulls":6},"□","平面図"]
[{"$nulls":15},"□","玄関（",null,"□","設置準備）",null,null,null,"□","脱衣室（",null,"（","□","設置準備）",null,null,"□","立面図"]
[{"$nulls":10},"転落防止手摺",null,null,null,"□","バルコニー",null,null,null,"（","□","手すりの設置",null,null,null,"□","転落のおそれなし）",{"$nulls":4},"□"]
[{"$nulls":10},"の設置",null,null,null,"□","窓（２階以上）",null,null,null,"（","□","手すりの設置",null,null,null,"□","転落のおそれなし）",{"$nulls":4},"□"]
[{"$nulls":10},"□","該当なし",null,null,"□","廊下及び階段"]
[{"$nulls":14},"（","□","開放なし",null,null,null,"□","手すりの設置",null,null,null,"□","転落のおそれなし）"]
[{"$nulls":14},"手すり子",null,null,"（","□","なし",null,null,"□","あり",null,null,"）"]
[{"$nulls":22},"内法寸法　",null,null,"□","110㎜以下"]
[{"$nulls":7},"通路等の",null,null,"通路の幅員",null,null,null,"□","通路有効幅員780㎜以上（柱等の箇所750㎜以上）",{"$nulls":15},"□","平面図"]
[{"$nulls":7},"幅員",null,null,"出入口の幅員",null,null,null,"□","玄関出入口の有効幅員750㎜以上",{"$nulls":15},"□"]
[{"$nulls":14},"□","浴室出入口の有効幅員600㎜以上"]
[{"$nulls":7},"(日常生活",{"$nulls":6},"□","玄関・浴室以外出入口の有効幅員750㎜以上"]
[{"$nulls":7},"空間内）",{"$nulls":7},"（","□","軽微な改造により確保",{"$nulls":6},"）"]
[{"$nulls":7},"寝室、便",null,null,"浴室の寸法",null,null,null,"□","内法面積2.0㎡、短辺内法寸法1,300㎜以上",{"$nulls":15},"□","平面図"]
[{"$nulls":7},"所及び浴",null,null,"便所の寸法等",null,null,null,"□","長辺内法寸法の1,300㎜以上",{"$nulls":15},"□"]
[{"$nulls":7},"室",{"$nulls":6},"もしくは"]
[{"$nulls":7},"(日常生活",{"$nulls":6},"□","便器と壁の距離が500㎜以上",{"$nulls":7},"（前方又は側方）"]
[{"$nulls":7},"空間内）",{"$nulls":6},"（","□","ドアの開放により確保",{"$nulls":5},"□","軽微な改造により確保",{"$nulls":6},"）"]
[{"$nulls":14},"□","腰掛け式便器を設置"]
[{"$nulls":10},"特定寝室面積",null,null,null,"□","特定寝室の内法面積9㎡以上"]

{"sheet":"高齢者等級4","index":5,"n_rows":44,"n_cols":37,"rows_kept":44,"cut":false,"hidden":false,"merged":[[43,7,43,9],[43,10,43,13],[14,21,14,25],[17,14,17,30],[37,7,37,9],[37,10,37,13],[38,7,38,9],[38,15,38,30],[38,10,38,13],[14,27,14,30],[40,7,40,9],[41,7,41,9],[40,15,40,21],[26,10,26,13],[27,10,27,13],[28,10,28,13],[30,14,30,16],[30,19,30,21],[32,7,32,9],[32,10,32,13],[23,10,23,13],[24,7,24,9],[24,10,24,13],[25,32,25,34],[21,10,21,13],[38,32,38,34],[30,23,30,25],[35,7,35,9],[35,10,35,13],[36,7,36,9],[15,10,15,13],[16,7,16,9],[17,32,17,34],[14,16,14,19],[13,10,13,13],[18,32,18,34],[12,10,12,13],[12,32,12,34],[13,32,13,34],[9,7,9,9],[9,10,9,13],[9,32,9,34],[8,19,8,20],[8,24,8,29],[9,1,9,4],[10,1,10,4],[11,7,11,9],[11,10,11,13],[27,32,27,34],[1,0,1,13],[1,14,1,36],[2,0,2,13],[2,14,2,36],[4,0,4,6],[4,8,4,34],[8,0,20,0],[8,7,8,9],[8,10,8,13],[6,35,7,36],[7,1,7,4],[7,7,7,9],[7,10,7,13],[7,14,7,30],[7,31,7,34],[6,1,6,4],[6,5,7,6],[6,7,6,9],[32,15,32,30],[33,7,33,9],[33,10,33,13],[6,10,6,34],[33,32,33,34],[31,22,31,24],[26,26,26,30],[29,26,29,30],[26,32,26,34],[27,26,27,30]],"flags":["formulas_cached_only"]}
["設計内容説明書【高齢者】",{"$nulls":35},"現金取得者向け新築対象住宅証明書用"]
["評価対象建築物の名称"]
["評価対象建築物の所在地"]
[]
["対象とする証明基準",{"$nulls":6},"■","　評価方法基準第5　9　9-1（3）【高齢者等配慮対策等級】　等級４"]
[]
[null,"性能表示　　　　",null,null,null,"自己\n評価\n結果",null,"確認",null,null,"設計内容説明欄",{"$nulls":24},"設計\n内容\n確認欄"]
[null,"事項",{"$nulls":5},"項目",null,null,"項目",null,null,null,"設計内容",{"$nulls":16},"記載図書"]
["９高齢者等への配慮","９－１",null,null,null,"等級",null,"部屋の",null,null,"特定寝室",null,null,null,"・","特定寝室",null,null,"（",null,null,"階、室名：",{"$nulls":8},"）","□","平面図"]
[null,"高齢者等配",null,null,null,"■",4,"配置等",null,null,"の位置",null,null,null,"□","便所",{"$nulls":15},"□"]
[null,"慮対策等級",{"$nulls":12},"□","浴室",null,"（基準に適合するエレベーター",{"$nulls":7},"□","有","）"]
[null,"（専用部分）",{"$nulls":5},"段差",null,null,"日常生活",null,null,null,"□","日常生活空間内の床が段差のない構造",{"$nulls":15},"□","平面図"]
[{"$nulls":10},"空間内",null,null,null,"・","適用除外の段差",{"$nulls":15},"□"]
[{"$nulls":15},"□","玄関出入口",null,null,null,"□","玄関上りかまち",{"$nulls":4},"□","浴室出入口"]
[{"$nulls":15},"□","勝手口出入口",null,null,null,"□","バルコニー出入口",{"$nulls":4},"□","ﾀﾀﾐｺｰﾅｰ"]
[{"$nulls":10},"日常生活空間外",null,null,null,"□","日常生活空間外の床が段差のない構造"]
[{"$nulls":7},"階段",null,null,"勾配等",null,null,null,"□","階段の勾配等の基準に適合",{"$nulls":15},"□","平面図"]
[{"$nulls":14},"　　　勾配6/7以下、550㎜≦けあげ×2＋踏面≦650㎜",{"$nulls":16},"□"]
[{"$nulls":7},"□","階段無",null,"蹴込み",null,null,null,"□","蹴込みが30mm以下、かつ、蹴込み板が設けられている",{"$nulls":15},"□"]
[{"$nulls":10},"形式等",null,null,null,"□","回り階段等安全上問題があると考えられる形式を用いていない"]
[{"$nulls":14},"□","通路等への食い込み及び突出が設けられていない"]
[{"$nulls":10},"除外規定",null,null,null,"□","ﾎｰﾑｴﾚﾍﾞｰﾀｰを設置し、かつ、等級3の階段の基準に適合"]
[{"$nulls":14},"□","日常生活空間外の階段で、かつ、等級3の階段の基準に適合"]
[{"$nulls":10},"階段の幅員等",null,null,null,"□","建築基準法施行令第23条から第27条までに定める基準に適合"]
[{"$nulls":7},"手摺",null,null,"手摺の設置",{"$nulls":4},"□","階段",null,null,"□","便所",null,null,"□","浴室",{"$nulls":6},"□","平面図"]
[{"$nulls":15},"□","玄関",null,null,"□","脱衣室",{"$nulls":10},"□"]
[{"$nulls":10},"転落防止手摺",null,null,null,"□","バルコニー",null,null,null,"（","□","手すりの設置",null,null,null,"□","転落のおそれなし）",{"$nulls":4},"□"]
[{"$nulls":10},"の設置",null,null,null,"□","窓（２階以上）",null,null,null,"（","□","手すりの設置",null,null,null,"□","転落のおそれなし）",{"$nulls":4},"□"]
[{"$nulls":14},"□","廊下及び階段"]
[{"$nulls":14},"（","□","開放なし",null,null,null,"□","手すりの設置",null,null,null,"□","転落のおそれなし）"]
[{"$nulls":14},"手すり子",null,null,"（","□","なし",null,null,"□","あり",null,null,"）"]
[{"$nulls":22},"内法寸法　",null,null,"□","110㎜以下"]
[{"$nulls":7},"通路等の",null,null,"通路の幅員",null,null,null,"□","通路有効幅員780㎜以上（柱等の箇所750㎜以上）",{"$nulls":15},"□","平面図"]
[{"$nulls":7},"幅員",null,null,"出入口の幅員",null,null,null,"□","玄関出入口の有効幅員750㎜以上",{"$nulls":15},"□"]
[{"$nulls":14},"□","浴室出入口の有効幅員650㎜以上"]
[{"$nulls":7},"(日常生活",{"$nulls":6},"□","玄関・浴室以外出入口の有効幅員750㎜以上"]
[{"$nulls":7},"空間内）",{"$nulls":7},"（","□","工事を伴わない撤去等",{"$nulls":11},"）"]
[{"$nulls":7},"寝室、便",null,null,"浴室の寸法",null,null,null,"□","内法面積2.5㎡、短辺内法寸法1,400㎜以上",{"$nulls":15},"□","平面図"]
[{"$nulls":7},"所及び浴",null,null,"便所の寸法等",null,null,null,"□","短辺内法寸法1,100㎜以上かつ長辺内法寸法の1,300㎜以上",{"$nulls":15},"□"]
[{"$nulls":7},"室",{"$nulls":6},"もしくは"]
[{"$nulls":7},"(日常生活",{"$nulls":6},"□","便器と壁の距離が500㎜以上",{"$nulls":7},"（前方及び側方）"]
[{"$nulls":7},"空間内）",{"$nulls":7},"□","ドアの開放により確保",{"$nulls":6},"□","軽微な改造により確保"]
[{"$nulls":14},"□","腰掛け式便器を設置"]
[{"$nulls":10},"特定寝室面積",null,null,null,"□","特定寝室の内法面積12㎡以上"]

{"sheet":"高齢者等級5","index":6,"n_rows":45,"n_cols":37,"rows_kept":45,"cut":false,"hidden":false,"merged":[[39,32,39,34],[42,7,42,9],[44,7,44,9],[44,10,44,13],[30,26,30,30],[31,14,31,16],[31,19,31,21],[31,23,31,25],[32,22,32,24],[33,15,33,30],[8,0,20,0],[14,16,14,19],[14,21,14,25],[14,27,14,30],[17,14,17,30],[18,32,18,34],[12,10,12,13],[12,32,12,34],[13,10,13,13],[13,32,13,34],[39,7,39,9],[41,7,41,9],[36,7,36,9],[36,10,36,13],[37,7,37,9],[38,10,38,13],[39,10,39,13],[38,7,38,9],[33,7,33,9],[33,10,33,13],[34,7,34,9],[34,10,34,13],[34,32,34,34],[27,32,27,34],[28,10,28,13],[29,10,29,13],[27,10,27,13],[27,26,27,30],[28,26,28,30],[28,32,28,34],[15,10,15,13],[16,7,16,9],[17,32,17,34],[25,10,25,13],[23,10,23,13],[24,10,24,13],[25,7,25,9],[26,32,26,34],[9,7,9,9],[9,10,9,13],[9,32,9,34],[10,1,10,4],[11,7,11,9],[11,10,11,13],[9,1,9,4],[8,7,8,9],[8,10,8,13],[8,19,8,20],[8,24,8,29],[1,0,1,13],[1,14,1,36],[2,0,2,13],[2,14,2,36],[4,0,4,6],[4,8,4,34],[6,35,7,36],[7,1,7,4],[7,7,7,9],[7,10,7,13],[7,14,7,30],[7,31,7,34],[6,1,6,4],[6,5,7,6],[6,7,6,9],[6,10,6,34]],"flags":["formulas_cached_only"]}
["設計内容説明書【高齢者】",{"$nulls":35},"現金取得者向け新築対象住宅証明書用"]
["評価対象建築物の名称"]
["評価対象建築物の所在地"]
[]
["対象とする証明基準",{"$nulls":6},"■","　評価方法基準第5　9　9-1（3）【高齢者等配慮対策等級】　等級５"]
[]
[null,"性能表示　　　　",null,null,null,"自己\n評価\n結果",null,"確認",null,null,"設計内容説明欄",{"$nulls":24},"設計\n内容\n確認欄"]
[null,"事項",{"$nulls":5},"項目",null,null,"項目",null,null,null,"設計内容",{"$nulls":16},"記載図書"]
["９高齢者等への配慮","９－１",null,null,null,"等級",null,"部屋の",null,null,"特定寝室",null,null,null,"・","特定寝室",null,null,"（",null,null,"階、室名：",{"$nulls":8},"）","□","平面図"]
[null,"高齢者等配",null,null,null,"■",5,"配置等",null,null,"の位置",null,null,null,"□","玄関",null,null,"□","便所",null,null,"□","浴室",null,null,"□","食事室",null,null,null,"□"]
[null,"慮対策等級",{"$nulls":12},"□","脱衣室及び洗面所",{"$nulls":4},"（基準に適合するエレベーター",{"$nulls":7},"□","有","）"]
[null,"（専用部分）",{"$nulls":5},"段差",null,null,"日常生活",null,null,null,"□","日常生活空間内の床が段差のない構造",{"$nulls":15},"□","平面図"]
[{"$nulls":10},"空間内",null,null,null,"・","適用除外の段差",{"$nulls":15},"□"]
[{"$nulls":15},"□","玄関出入口",null,null,null,"□","玄関上りかまち"]
[{"$nulls":15},"□","勝手口出入口",null,null,null,"□","バルコニー出入口",{"$nulls":4},"□","ﾀﾀﾐｺｰﾅｰ"]
[{"$nulls":10},"日常生活空間外",null,null,null,"□","日常生活空間外の床が段差のない構造"]
[{"$nulls":7},"階段",null,null,"勾配等",null,null,null,"□","階段の勾配等の基準に適合",{"$nulls":15},"□","平面図"]
[{"$nulls":14},"　　　勾配6/7以下、550㎜≦けあげ×2＋踏面≦650㎜",{"$nulls":16},"□"]
[{"$nulls":7},"□","階段無",null,"蹴込み",null,null,null,"□","蹴込みが30mm以下、かつ、蹴込み板が設けられている",{"$nulls":15},"□"]
[{"$nulls":10},"形式等",null,null,null,"□","回り階段等安全上問題があると考えられる形式を用いていない"]
[{"$nulls":14},"□","通路等への食い込み及び突出が設けられていない"]
[{"$nulls":14},"□","滑り止め無し、又は滑り止めが踏面と同一面"]
[{"$nulls":14},"□","段鼻なし"]
[{"$nulls":10},"除外規定",null,null,null,"□","ﾎｰﾑｴﾚﾍﾞｰﾀｰを設置し、かつ、等級3の階段の基準に適合"]
[{"$nulls":10},"階段の幅員等",null,null,null,"□","建築基準法施行令第23条から第27条までに定める基準に適合"]
[{"$nulls":7},"手摺",null,null,"手摺の設置",{"$nulls":4},"□","階段",null,null,"□","便所",null,null,"□","浴室",{"$nulls":6},"□","平面図"]
[{"$nulls":15},"□","玄関",null,null,"□","脱衣室",{"$nulls":10},"□"]
[{"$nulls":10},"転落防止手摺",null,null,null,"□","バルコニー",null,null,null,"（","□","手すりの設置",null,null,null,"□","転落のおそれなし）",{"$nulls":4},"□"]
[{"$nulls":10},"の設置",null,null,null,"□","窓（２階以上）",null,null,null,"（","□","手すりの設置",null,null,null,"□","転落のおそれなし）",{"$nulls":4},"□"]
[{"$nulls":14},"□","廊下及び階段"]
[{"$nulls":14},"（","□","開放なし",null,null,null,"□","手すりの設置",null,null,null,"□","転落のおそれなし）"]
[{"$nulls":14},"手すり子",null,null,"（","□","なし",null,null,"□","あり",null,null,"）"]
[{"$nulls":22},"内法寸法　",null,null,"□","110㎜以下"]
[{"$nulls":7},"通路等の",null,null,"通路の幅員",null,null,null,"□","通路有効幅員850㎜以上（柱等の箇所800㎜以上）",{"$nulls":15},"□","平面図"]
[{"$nulls":7},"幅員",null,null,"出入口の幅員",null,null,null,"□","玄関出入口の有効幅員800㎜以上",{"$nulls":15},"□"]
[{"$nulls":14},"□","浴室出入口の有効幅員800㎜以上"]
[{"$nulls":7},"(日常生活",{"$nulls":6},"□","玄関・浴室以外出入口の有効幅員800㎜以上"]
[{"$nulls":7},"空間内）",{"$nulls":7},"（","□","工事を伴わない撤去等",{"$nulls":6},"）"]
[{"$nulls":7},"寝室、便",null,null,"浴室の寸法",null,null,null,"□","内法面積2.5㎡、短辺内法寸法1,400㎜以上",{"$nulls":15},"□","平面図"]
[{"$nulls":7},"所及び浴",null,null,"便所の寸法等",null,null,null,"短辺内法寸法",{"$nulls":16},"□"]
[{"$nulls":7},"室",{"$nulls":6},"□","1,300㎜以上",{"$nulls":6},"もしくは"]
[{"$nulls":7},"(日常生活",{"$nulls":6},"□","便器後方の壁から便器の先端までの距離＋500㎜以上"]
[{"$nulls":7},"空間内）",{"$nulls":7},"（","□","工事を伴わない撤去等",{"$nulls":6},"）"]
[{"$nulls":14},"□","腰掛け式便器を設置"]
[{"$nulls":10},"特定寝室面積",null,null,null,"□","特定寝室の内法面積12㎡以上"]